**Research Analysis**

**Electric Vehicle Population Analysis using Pandas and Matplotlib**

The rapid growth of electric vehicles (EVs) requires robust data analysis to support grid planning, charging infrastructure, and policy decisions. Research highlights the value of population-based and individual-based approaches in modeling EV charging behavior. **Ma & Callaway (2013)** demonstrate how decentralized charging control can effectively manage large EV populations, reducing grid stress and optimizing energy distribution. **Kovacevic et al. (2023)** extend this work by proposing aggregated representations of EV populations at charging points, which allow planners to analyze usage patterns with fewer computational resources.[1], [2], [3]

**Python**, with its data analysis libraries, offers a practical way to implement these concepts.

* **Pandas** handles large EV datasets- such as charging times, energy consumed, and geographic locations - by enabling filtering, grouping, and aggregation operations. This supports building population-level models similar to those in the cited studies.
* **Matplotlib** allows visualization of patterns such as hourly demand curves, regional charging hotspots, and adoption growth over time. This mirrors the graphical analyses used in EV research to identify system bottlenecks and behavioral trends.

**Key insights from the research papers combined with Python tools:**

* **Population-level modeling** simplifies analysis and supports scenario simulations, such as peak demand forecasting.[1]
* **Decentralized control approaches** can be tested with synthetic datasets to measure potential grid impact.
* **Visualization and exploratory analysis** enhance decision-making by revealing hidden trends.[4]
* **Data integration** with libraries like xarray allows working with multidimensional EV datasets such as time × location × power demand.[5]

**Practical outcome:**  
By combining Pandas’ data wrangling power with Matplotlib’s visualization capabilities, researchers and planners can create dashboards showing real-time or historical EV population data. This approach is cost-effective, reproducible, and scalable, making it ideal for supporting both academic research and government or industry decision-making.

**BIBLIOGRAPHY**

[1] A. F. Cortés Borray, J. Merino, E. Torres, and J. Mazón, “A review of the population-based and individual-based approaches for electric vehicles in network energy studies,” 2020. doi: 10.1016/j.epsr.2020.106785.

[2] Z. Ma, D. S. Callaway, and I. A. Hiskens, “Decentralized charging control of large populations of plug-in electric vehicles,” *IEEE Transactions on Control Systems Technology*, vol. 21, no. 1, 2013, doi: 10.1109/TCST.2011.2174059.

[3] M. Kovacevic and M. Vasak, “Aggregated Representation of Electric Vehicles Population on Charging Points for Demand Response Scheduling,” *IEEE Transactions on Intelligent Transportation Systems*, vol. 24, no. 10, 2023, doi: 10.1109/TITS.2023.3286012.

[4] K. Sahoo, A. K. Samal, J. Pramanik, and S. K. Pani, “Exploratory data analysis using python,” *International Journal of Innovative Technology and Exploring Engineering*, vol. 8, no. 12, 2019, doi: 10.35940/ijitee.L3591.1081219.

[5] S. Hoyer and J. Hamman, “xarray: N-D labeled Arrays and Datasets in Python,” *J Open Res Softw*, vol. 5, no. 1, 2017, doi: 10.5334/jors.148.